**Constants**

|  |  |  |  |
| --- | --- | --- | --- |
| Name | Description | Type | Value |
| commMoveBackward | Code sent to the robot to move backwards | Number | 0x02 |
| commMoveForward | Code sent to the robot to move forward | Number | 0x01 |
| commStop | Code sent to the robot to stop | Number | 0x00 |
| commTurnLeft | Code sent to the robot to move left | Number | 0x03 |
| commTurnRight | Code sent to the robot to move right | Number | 0x04 |
| errBadCommand | Error code: command sent that robot doesn’t recognize | Number | 0xFF02 |
| errBadSignal | Error code: robot not getting good signal from device | Number | 0xFF01 |
| errBatteryLow | Error code: robot batteries are low | Number | 0xFF03 |
| productName | String with the name of the physical product | String | RoboBall |
| versionNumber | SDK version number | Number | 1.6 |

**commMoveBackward**

Code sent to the robot to move backwards.

**commMoveForward**

Code sent to the robot to move forward.

**commStop**

Code sent to the robot to sto .

**commTurnLeft**

Code sent to the robot to move left.

**commTurnRight**

Code sent to the robot to move right.

**errBadCommand**

Error code: command sent that robot doesn’t recognize.

**errBadSignal**

Error code: robot not getting good signal from device.

**errBatteryLow**

Error code: robot batteries are low.

**productName**

String with the name of the physical product.

**versionNumber**

SDK version number.